SWPPP HQ
Weekly SWPPP inspection report (Detailed version)
Free template from SWPPP HQ, an independent site. Not an official SCDES, county, or MS4 form. Check your permit, SWPPP, and local MS4 for what's required.
Last updated: October 20, 2026
Sites in Anderson County: use Anderson County's own inspection report (Appendix H) instead of this template.
	Site

	Site Name
Required · 4.2.F.XI
	

	Operator Name
Required · 4.2.F.XI
	

	Permit number
Required · 4.2.F.XI
	

	Inspection

	The inspection date
Required · 4.2.F.I
	

	Date of previous inspection
Optional · 4.2.B
	

	Inspection basis
Optional · 4.2.B-C
	☐ Weekly (4.2.B)
☐ Monthly, stabilized portion (4.2.B)
☐ Linear site, representative inspection (4.2.C)
☐ More frequent, as required by SCDES (4.2.B)

	Portion of the site inspected by a Secondary Permittee
Optional · 4.2.A
	

	Inspector

	Names, titles, and, , the qualifications of personnel making the inspection if not previously given in an inspection report, unless those qualifications change
Required · 4.2.F.II
	



	Qualification basis
Optional · 4.2.E
	☐ Preparer of the C-SWPPP (4.2.E)
☐ Registration equivalent to the C-SWPPP preparer's (4.2.E)
☐ Under the direct supervision of a person qualified to prepare a C-SWPPP (4.2.E)
☐ Certified through a Construction Site Inspector Certification Course (4.2.E, last bullet)
☐ Project of 2 acres or less, not part of an LCP: Permittee or designee (4.2.E.I)

	Inspection

	Areas inspected
Optional · 4.2.A.I-V
	☐ All areas of the site disturbed by construction activity and areas used for storage of materials that are exposed to precipitation (4.2.A.I)
☐ All stormwater conveyance systems for any evidence of, or the potential for, pollutants entering these systems (4.2.A.II)
☐ All BMPs identified in the OS-SWPPP (4.2.A.III)
☐ All discharge locations to ascertain whether the implemented BMPs are effective in preventing the discharge of sediment from the site (4.2.A.IV)
☐ Locations where vehicles enter or exit the site must be inspected for evidence of off-site sediment tracking (4.2.A.V)

	Findings

	All discharge points
Required · 4.2.F.III
	



	Weather information and a description of any discharges occurring at the time of the inspection
Required · 4.2.F.IV
	



	Rainfall

	Total rainfall since last inspection
Required · 4.2.F.V
	

	Rainfall records for the day of the inspection
Required · 4.2.D
	

	Significant rainfall events (0.5 inches or greater) since the last inspection: dates and amounts
Required · 4.2.D
	


	Rainfall source
Optional · 4.2.D
	☐ On-site rain gauge (4.2.D)
☐ Certified weather record located within reasonable proximity of the construction site, such as a personal weather station or an airport (4.2.D)

	Findings

	Location(s) of discharges of sediment or other pollutants from the Site
Required · 4.2.F.VI
	



	Location(s) of BMPs that need maintenance
Required · 4.2.F.VII
	



	Location(s) of BMPs that failed to operate as designed or proved inadequate for a particular location
Required · 4.2.F.VIII
	



	Location(s) where additional BMPs are needed that did not exist at the time of inspection
Required · 4.2.F.IX
	



	Corrective action required including any changes to the OS-SWPPP necessary and implementation dates
Required · 4.2.F.X
	




	Verification that all BMPs and stormwater controls identified in the OS-SWPPP have been installed and are operating as designed.
Required · 4.2.F.XII
	☐ Yes    ☐ No    Notes:



	Determine if the construction sequence is being followed
Required · 4.2.F.XIII
	☐ Yes    ☐ No    Notes:



	Follow-up

	Status of corrective actions undertaken following previous inspection to include date(s) each item was addressed
Required · 4.2.F.XIV
	




	List of items that have carried over from previous inspection reports that were not addressed.
Required · 4.2.F.XV
	



	Signature

	Signature of the qualified inspector
Required · 4.2.H
	


Frequency: inspections "must be conducted at a minimum of at least once every calendar week, with no time period between inspections exceeding 9 days" (CGP 4.2.B).
Stabilized portions: frequency "may be reduced to at least once every month, as long as the stabilization is maintained and there is no additional disturbance in these areas" (CGP 4.2.B).
Keep: "A record of each inspection and of any actions taken in accordance with this Section must be retained as part of the On-site SWPPP for at least three years from the date that permit coverage expires or is terminated." (CGP 4.2.H; see also 7.1)
Free template from SWPPP HQ, an independent site. Not an official SCDES, county, or MS4 form. Check your permit, SWPPP, and local MS4 for what's required. Last updated: October 20, 2026




